# Epson Firmware Update Procedure

Pre-installation procedure

Connect the system to the printer and switch the Printer ON.

Download Nexxo.Epson.FirmwareUpdate.msi

Create a text file with the name NexxoConfig.txt files, having the following parameters

ClientID 33

InstallLogFolder G:\LOG\

InstallErrorFolder G:\LOG\

ServiceURL <https://172.18.100.222/Nexxo.Channel.DMS.NpsInstallerServer.Svc_HttpsTest/NpsInstallerWSImpl.svc>

ClientId will be used only during the NPS Installation. The configuration file is common for both installs. Log folder can be a shared location also.

Run Nexxo.Epson.FirmwareUpdate.msi

After the firmware update, printer would be reset.   
But please confirm, firmware has been updated by self test print. (Turn off printer. Turn on printer while keep pressing FEED button)   
The version should be 1.06 ESC/POS.

After the above process, Power Cycle the Printer again.

For Remote Installation, follow the same procedure specified for Epson Driver Installation by creating a new Policy Object.